* We evaluate scheduling of high performance applications on asymmetric multi-cores
* We compare three scheduling approaches taking place on different levels of the software stack
* We analyze the results in terms of: performance, energy consumption and power
* We find that the runtime system is the most appropriate level for scheduling on asymmetric multicores
* We investigate different runtime scheduling approaches (e.g. loop vs task-based)